|  |  |  |  |
| --- | --- | --- | --- |
| **Vehicle description:** |  | **Inspection Date:** |  |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Rego No:** |  | **Fleet No:** |  | **RUC label kms:** |  |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Service Due – date:** |  | **Rego Due:** |  | **Odo kms:** |  |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Service Due – kms:** |  | **WOF Due:** |  | **RUC kms remaining:** |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **No.** | **Item** | **Ok?** | **Comments** |
| **1** | Bodywork, doors, lights, running boards undamaged & secure |  |  |
| **2** | Structural after-market modifications (rollover protection / bull-bars etc.) certified, undamaged & secure |  |  |
| **3** | Non-structural after-market modifications (auxiliary lights, aerials etc.) undamaged & secure |  |  |
| **4** | Wheels, wheel-nuts, tyres, mud flaps undamaged & secure |  |  |
| **5** | Tyres correctly inflated, >5mm tread depth, wearing evenly |  |  |
| **6** | Tow ball, trailer electrical connector undamaged & secure |  |  |
| **7** | Cab interior hygienic, uncluttered with no unsecured objects |  |  |
| **8** | Seats and seat belts undamaged & functioning correctly |  |  |
| **9** | Mirrors clear, secure, & correctly positioned |  |  |
| **10** | Dash gauges, warning lights, reversing camera/alarm operational |  |  |
| **11** | Lights, horn, indicators, hazard lights operational |  |  |
| **12** | Windows clear, control mechanisms & wipers functional |  |  |
| **13** | Fire extinguisher easily accessible, in-test & secure |  |  |
| **14** | 1st aid kit easily accessible, adequately stocked & secure |  |  |
| **15** | Engine oil level |  |  |
| **16** | Transmission oil level |  |  |
| **17** | Engine coolant level |  |  |
| **18** | Window washer bottle full |  |  |
| **19** | Mechanical servicing in accordance with manufacturers specifications |  |  |

|  |  |
| --- | --- |
| **Vehicle fit for use:** | **Yes / No** |
| **Inspector name:** | **Signature:** |